{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["水溶液","原子量・Victreen係数表","溶液試料判定"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"水溶液","index":0,"n_rows":19,"n_cols":6,"rows_kept":19,"cut":false,"hidden":true,"merged":[[2,3,3,5]]}
[null,"Ci","Di","λ","Cj","Dj"]
["標的元素のビクトリーン係数",176,48.3,1.38,15.6,0.77900000000000003]
["H のビクトリーン係数",1.2699999999999999E-2,4.6600000000000003E-6,"←水溶液とみなすため固定"]
["O のビクトリーン係数",3.18,6.54E-2]
["標的原子の原子量 [g/mol]",63.545999999999999]
["試料の濃度[mol/l ,M]",1]
["試料の厚さ [cm]",0.1]
["試料の密度(重量分率) [g/cm3]",{"$f":"B6*B5/1000","v":6.3546000000000005E-2}]
["μM(lowE) [cm2/g]",{"$f":"E2*D2^3-F2*D2^4","v":38.172693238559987}]
["μM(highE) [cm2/g]",{"$f":"B2*D2^3-C2*D2^4","v":287.36916091199998}]
["μM(H2O) [cm2/g]",{"$f":"(B3*D2^3-C3*D2^4)*(2/18)+(B4*D2^3-C4*D2^4)*(16/18)","v":7.221555695626952}]
[]
["μM(lowE)",{"$f":"(B11*(1-B8)+B9*B8)*1*B7","v":0.91883766819301749}]
["μM(highE)",{"$f":"ROUND((B11*(1-B8)+B10*B8)*1*B7,3)","v":2.5019999999999998},{"$f":"IF(B14>4,\"OUT\",\"SAFE\")","v":"SAFE"}]
["⊿μM",{"$f":"ROUND(B14-B13,3)","v":1.583},{"$f":"IF(OR(B15>2),\"OUT\",\"SAFE\")","v":"SAFE"},null,"総合判定",{"$f":"IF(AND(C14=\"SAFE\",C15=\"SAFE\"),\"SAFE\",\"OUT\")","v":"SAFE"}]
[]
[]
["上限のサンプル厚さ[cm]",{"$f":"ROUND(4/(B11*(1-B8)+B10*B8),3)","v":0.16}]
["(μt≦4になるときの厚さ)"]

{"sheet":"原子量・Victreen係数表","index":1,"n_rows":84,"n_cols":9,"rows_kept":84,"cut":false,"hidden":true,"merged":[]}
["原子番号","元素名","原子量","Ci","Di","λabs","Cj","Dj","Edge"]
[1,"H",1.0079400000000001,1.2699999999999999E-2,4.6600000000000003E-6,null,null,null,"K"]
[2,"He",4.0026020000000004,5.1400000000000001E-2,7.5199999999999998E-5,null,null,null,"K"]
[3,"Li",6.9409999999999998,0.15,4.9399999999999997E-4,null,null,null,"K"]
[4,"Be",9.0121819999999992,0.36499999999999999,2.1299999999999999E-3,null,null,null,"K"]
[5,"B",10.811,0.60899999999999999,4.5100000000000001E-3,null,null,null,"K"]
[6,"C",12.0107,1.22,1.4200000000000001E-2,null,null,null,"K"]
[7,"N",14.006740000000001,2.0499999999999998,3.1699999999999999E-2,null,null,null,"K"]
[8,"O",15.9994,3.18,6.54E-2,null,null,null,"K"]
[9,"F",18.998403199999998,4.5999999999999996,0.112,null,null,null,"K"]
[10,"Ne",20.1797,6.51,0.20599999999999999,null,null,null,"K"]
[11,"Na",22.98977,8.67,0.33,null,null,null,"K"]
[12,"Mg",24.305,11.3,0.53900000000000003,9.5116999999999994,null,null,"K"]
[13,"Al",26.981538,14.4,0.80300000000000005,7.9511000000000003,null,null,"K"]
[14,"Si",28.0855,18.2,1.1000000000000001,6.7446000000000002,null,null,"K"]
[15,"P",30.973761,22.6,1.55,5.7885999999999997,null,null,"K"]
[16,"S",32.066000000000003,27.6,2.1800000000000002,5.0182000000000002,null,null,"K"]
[17,"Cl",35.4527,33.4,3.03,4.3968999999999996,null,null,"K"]
[18,"Ar",39.948,40,4.18,3.8706999999999998,null,null,"K"]
[19,"K",39.098300000000002,47.4,5.59,3.4363999999999999,null,null,"K"]
[20,"Ca",40.078000000000003,55.8,7.56,3.0701999999999998,null,null,"K"]
[21,"Sc",44.955910000000003,65.2,9.81,2.7570000000000001,null,null,"K"]
[22,"Ti",47.887,75.599999999999994,12.3,2.4969999999999999,5.15,0.153,"K"]
[23,"V",50.941499999999998,86.9,15.1,2.2690000000000001,6.14,0.20300000000000001,"K"]
[24,"Cr",51.996099999999998,99,18.2,2.0699999999999998,7.24,0.26800000000000002,"K"]
[25,"Mn",54.938048999999999,112,22.3,1.8959999999999999,8.51,0.34399999999999997,"K"]
[26,"Fe",55.844999999999999,126,27.2,1.7430000000000001,9.9499999999999993,0.433,"K"]
[27,"Co",58.933199999999999,141,33.200000000000003,1.6080000000000001,11.6,0.53500000000000003,"K"]
[28,"Ni",58.693399999999997,158,40.1,1.488,13.4,0.65100000000000002,"K"]
[29,"Cu",63.545999999999999,176,48.3,1.38,15.6,0.77900000000000003,"K"]
[30,"Zn",65.39,195,57.7,1.2829999999999999,17.8,0.93700000000000006,"K"]
[31,"Ga",69.722999999999999,216,68.599999999999994,1.196,20.2,1.1299999999999999,"K"]
[32,"Ge",72.61,238,81.099999999999994,1.117,22.7,1.37,"K"]
[33,"As",74.921599999999998,262,95.4,1.0449999999999999,25.3,1.67,"K"]
[34,"Se",78.959999999999994,287,112,0.98,28,2.02,"K"]
[35,"Br",79.903999999999996,314,130,0.92,30.9,2.4300000000000002,"K"]
[36,"Kr",83.8,343,151,0.86550000000000005,33.9,2.92,"K"]
[37,"Rb",85.467799999999997,374,174,0.8155,37.1,3.48,"K"]
[38,"Sr",87.62,406,200,0.76970000000000005,40.5,4.1399999999999997,"K"]
[39,"Y",88.905850000000001,441,229,0.72760000000000002,44.1,4.88,"K"]
[40,"Zr",91.224000000000004,477,261,0.68879999999999997,47.9,5.72,"K"]
[41,"Nb",92.906379999999999,515,296,0.65290000000000004,51.9,6.67,"K"]
[42,"Mo",95.94,555,336,0.61980000000000002,56.2,7.73,"K"]
[43,"Tc",null,597,379,0.58909999999999996,60.7,8.91,"K"]
[44,"Ru",101.07,641,427,0.56000000000000005,65.5,10.1,"K"]
[45,"Rh",102.9055,686,479,0.53400000000000003,70.5,11.4,"K"]
[46,"Pd",106.42,734,537,0.50900000000000001,75.8,12.8,"K"]
[47,"Ag",107.8682,784,599,0.48599999999999999,81.400000000000006,14.3,"K"]
[48,"Cd",112.411,835,667,0.46400000000000002,87.4,15.9,"K"]
[49,"In",114.818,889,741,0.44400000000000001,93.6,17.7,"K"]
[50,"Sn",118.71,944,821,0.42499999999999999,100,19.7,"K"]
[51,"Sb",121.76,1000,908,0.40660000000000002,107,21.8,"K"]
[52,"Te",127.6,1060,1000,0.38969999999999999,114,24.3,"K"]
[53,"I",126.90447,1120,1100,0.37380000000000002,122,27.1,"K"]
[54,"Xe",131.29,1180,1210,0.35849999999999999,130,30.2,"K"]
[55,"Cs",132.90545,51.7,6.87,2.4739,17,1.38,"L3"]
[56,"Ba",137.327,56.3,7.86,2.3628,19.2,1.72,"L3"]
[57,"La",138.90549999999999,61.2,8.9600000000000009,2.2582,21.5,2.0699999999999998,"L3"]
[58,"Ce",140.11500000000001,66.3,10.199999999999999,2.1638999999999999,23.8,2.44,"L3"]
[59,"Pr",140.90764999999999,71.7,11.5,2.077,26.1,2.83,"L3"]
[60,"Nd",144.24,77.400000000000006,13,1.9946999999999999,28.4,3.24,"L3"]
[61,"Pm",null,83.3,14.7,1.917,30.7,3.67,"L3"]
[62,"Sm",150.36000000000001,89.6,16.5,1.8445,33.1,4.12,"L3"]
[63,"Eu",151.964,96.1,18.5,1.7753000000000001,35.4,4.6100000000000003,"L3"]
[64,"Gd",157.25,103,20.7,1.7094,37.799999999999997,5.1100000000000003,"L3"]
[65,"Tb",158.92534000000001,110,23.1,1.6486000000000001,40.299999999999997,5.64,"L3"]
[66,"Dy",162.5,118,25.7,1.579,42.8,6.2,"L3"]
[67,"Ho",164.93031999999999,125,28.5,1.5353000000000001,45.4,6.79,"L3"]
[68,"Er",167.26,133,31.6,1.4822,48,7.41,"L3"]
[69,"Tm",168.93421000000001,142,34.799999999999997,1.4328000000000001,50.7,8.06,"L3"]
[70,"Yb",173.04,151,38.4,1.3861000000000001,53.4,8.75,"L3"]
[71,"Lu",174.96700000000001,160,42.2,1.3413999999999999,56.2,9.4700000000000006,"L3"]
[72,"Hf",178.49,169,46.2,1.2970999999999999,59.2,10.199999999999999,"L3"]
[73,"Ta",180.9479,179,50.5,1.2551000000000001,62.2,11,"L3"]
[74,"W",183.84,190,55.2,1.2154,65.3,11.9,"L3"]
[75,"Re",186.20699999999999,200,60.1,1.177,68.400000000000006,12.7,"L3"]
[76,"Os",190.23,212,65.400000000000006,1.1404000000000001,71.8,13.6,"L3"]
[77,"Ir",192.21700000000001,223,70.900000000000006,1.1055999999999999,75.2,14.6,"L3"]
[78,"Pt",195.078,235,76.8,1.0724,78.7,15.6,"L3"]
[79,"Au",196.96655000000001,247,83,1.0399,82.3,16.600000000000001,"L3"]
[80,"Hg",200.59,260,89.6,1.0089999999999999,86.1,17.7,"L3"]
[81,"Tl",204.38329999999999,274,96.6,0.97929999999999995,90,18.899999999999999,"L3"]
[82,"Pb",207.2,287,104,0.95030000000000003,94.1,20,"L3"]
[83,"Bi",208.98038,302,112,0.9234,98.3,21.3,"L3"]

{"sheet":"溶液試料判定","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}